; Windows 2000, XP & Vista setup File for AVR CDC Device
[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%ATMEL% <Replace ATMEL by your manufacture name>
DriverVer=10/15/1999,5.0.2153.1
;----------------------------------------------------------
; Targets
;----------------------------------------------------------
[Manufacturer]
%ATMEL%=ATMEL, NTamd64 <Replace ATMEL by your manufacture name>
[ATMEL]
%ATMEL_CDC%=Reader, USB\VID_03EB&PID_2404
<Replace 03EB by your VID, Replace 2404 by your PID>
[ATMEL.NTamd64]
%ATMEL_CDC%=DriverInstall, USB\VID_03EB&PID_2404
<Replace 03EB by your VID, Replace 2404 by your PID>
;----------------------------------------------------------
; Windows 2K, XP, and Vista32
;----------------------------------------------------------
[Reader_Install.NTx86]
[DestinationDirs]
DefaultDestDir=12
Reader.NT.Copy=12
[Reader.NT]
include=mdmcpq.inf
CopyFiles=Reader.NT.Copy
AddReg=Reader.NT.AddReg
[Reader.NT.Copy]
usbser.sys
[Reader.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
[Reader.NT.Services]
AddService = usbser, 0x00000002, Service_Inst
[Service_Inst]
DisplayName = %Serial.SvcDesc%
ServiceType = 1 ; SERVICE_KERNEL_DRIVER
StartType = 3 ; SERVICE_DEMAND_START
ErrorControl = 1 ; SERVICE_ERROR_NORMAL
ServiceBinary = %12%\usbser.sys
LoadOrderGroup = Base
;----------------------------------------------------------
; Vista64
;----------------------------------------------------------
[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg
[DriverCopyFiles.NTamd64]
usbser.sys,,,0x20
[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService.NTamd64
[DriverService.NTamd64]
DisplayName=%Serial.SvcDesc%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys
;----------------------------------------------------------
; String
;----------------------------------------------------------
[Strings]
ATMEL = "ATMEL, Inc." <Replace ATMEL by your manufacture name>
ATMEL_CDC = "AVR Communication Device Class"
<Write your device description>
Serial.SvcDesc = "USB Serial emulation driver"